PiRail

A raspberry pi controlled model railway

Contents

[General Overview 1](#_Toc505770837)

[Websocket Protocol 1](#_Toc505770838)

[Admin Controls (0x80 Flag) 2](#_Toc505770839)

[Train (0x40 Flag) 3](#_Toc505770840)

[Track (0x20 Flag) 4](#_Toc505770841)

[General (0x10 Flag) 4](#_Toc505770842)

[Circuit of RNet 5](#_Toc505770843)

[Protocol of RNet 5](#_Toc505770844)

[General 5](#_Toc505770845)

[Output 5](#_Toc505770846)

[Input 7](#_Toc505770847)

[Set Device Parameters 8](#_Toc505770848)

[EEPROM on Arduino 9](#_Toc505770849)

# General Overview



# Websocket Protocol

Each Websocket message is send as a binary packet.

You can register to certain topics as a Websocket client using the protocol properties. 255 registers you to all the topics.

The messages are divided into 4 different categories. The system checks for the first set bit. The packet belong to a category if the first bit equals the flag.

## Admin Controls (0x80 Flag)

### Clear track

Delete all the track from current layout.

0x80

### Reload track

Rescan the track for modules. They still need to be ‘joined’ together.

0x81

### Reload Previous track

Reload a layout from a previous setup. They don’t have to be ‘joined’ together

0x82

### Reset Switches

Reset all switches to default

0x83

### Toggle (Light) Output

Toggle output of modules on or off.

0x84

### All train back to depot

Send all trains back to depot, only if depot space is available.

0x88

### Force Switch

Force a switch to a state independent of reserved state.

0xA0

### Emergency Stop, Admin authority

Set emergency stop. Can only be release with admin authority (the send code).

0x90 Admin Code 2 bytes (0-65534)

### Emergency Release, Admin authority

Release Emergency stop.

0x91 Admin Code 2 bytes (0-65534)

## Train (0x40 Flag)

### Set new train

0x40

### Speed control

0x41

### Function control

0x42

### Operation change

0x43

### Add Route

0x44

### Delete Route

0x45

## Track (0x20 Flag)

### Toggle Switch

0x20

### MSSwitch toggle up

0x21

### MSSwitch toggle down

0x22

### Set switch

0x23

### Set switch reserved

0x24

## General (0x10 Flag)

### Emergency stop

Set emergency stop, can be released by everyone

0x10

### Emergency stop

Release emergency stop. Can release emergency stop commenced by admin

0x11

### New Message

0x12

### Message Clear

0x13

# Circuit of RNet

There are 4 RNet devices in the network: COM interface, RNet controller, RNet output module, RNet input module.

# Protocol of RNet

## General

### Report ID

|  |  |  |
| --- | --- | --- |
| 0x00 | DevID | Checksum |

All devices sends this packet at startup, so that the controller knows which modules are present.

### Set Emergency STOP

|  |  |
| --- | --- |
| 0x01 | Checksum |

### Release Emergency STOP

|  |  |
| --- | --- |
| 0x02 | Checksum |

### Set Power ON

|  |  |
| --- | --- |
| 0x03 | Checksum |

### Set Power OFF

|  |  |
| --- | --- |
| 0x04 | Checksum |

### Set Acknowledge

|  |  |  |
| --- | --- | --- |
| 0x7F | DevID | Checksum |

## Output

### Toggle Single Address

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 0x10 | DevID | Output Low | Output High | Checksum |

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

Toggles the output of the specified ID.

### Pulse Single Address

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 0x11 | DevID | Output Low | Output High | Checksum |

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

Send a pulse on the output of the specified ID.

### Toggle Blink Single Address

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 0x12 | DevID | Output Low | Output High | Checksum |

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

Toggles the output of the specified ID.

### Toggle Multiple Addresses

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x13 | Length | DevID | Output1 Low | Output1 High | … | Checksum |

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

Toggles multiple addresses

### Set All output Addresses

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x14 | Length | DevID | Output1 | Output2 | … | Checksum |

Output1: Output & 0x7F  
Output2: (Output >> 7) & 0x7F  
Output3: (Output >> 14) & 0x7F

Set all output to the specified bytes. Output 1 contains the ID of 0-6, output 2 contains 7-13, and so on. NOT IMPLEMENTED

### Set Blink mask of all addresses

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x15 | Length | DevID | Output1 | Output2 | … | Checksum |

Output1: Output & 0x7F  
Output2: (Output >> 7) & 0x7F  
Output3: (Output >> 14) & 0x7F

Set the blink mask to the specified bytes. Output 1 contains the ID of 0-6, output 2 contains 7-13, and so on. NOT IMPLEMENTED

### Post all Output

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x16 | Length | DevID | Output1 | Output2 | … | Checksum |

Output1: Output & 0x7F  
Output2: (Output >> 7) & 0x7F  
Output3: (Output >> 14) & 0x7F

### Request Read all Output

|  |  |  |
| --- | --- | --- |
| 0x47 | DevID | Checksum |

***Response:*** Post all Output (0x07)

## Input

### Post Single Input Address

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 0x05 | DevID | Output Low | Output High | Checksum |

DevID: ID & 0x7F

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

### Post Multiple Addresses

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x06 | Length | DevID | Output1 Low | Output1 High | … | Checksum |

DevID: ID & 0x7F

Output Low: ID & 0x7F  
Output High: (ID >> 7) & 0x7F

### Post All input Addresses

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x07 | Length | DevID | Output1 | Output2 | … | Checksum |

DevID: ID & 0x7F

Output1: Output & 0x7F  
Output2: (Output >> 7) & 0x7F  
Output3: (Output >> 14) & 0x7F

### Post all Input

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x08 | Length | DevID | Output1 | Output2 | … | Checksum |

DevID: ID & 0x7F

Output1: Output & 0x7F  
Output2: (Output >> 7) & 0x7F  
Output3: (Output >> 14) & 0x7F

### Request Read all Inputs

|  |  |  |
| --- | --- | --- |
| 0x4C | DevID | Checksum |

DevID: ID & 0x7F

***Response:*** Post all Input (0x07)

## Set Device Parameters

***The device acknowledges all the changes to its parameters with the acknowledge packet***

### Change Device ID

|  |  |  |  |
| --- | --- | --- | --- |
| 0x50 | Old DevID | New DevID | Checksum |

### Set number of input modules and output modules

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 0x51 | DevID | Input Modules | Output Modules | Checksum |

### Set blink Interval

|  |  |  |  |
| --- | --- | --- | --- |
| 0x52 | DevID | Interval scalar | Checksum |

Blink interval (ms) =

### Set Pulse length

|  |  |  |  |
| --- | --- | --- | --- |
| 0x53 | DevID | Pulse scalar | Checksum |

Pulse duration (ms) =

### Set Check input Interval

|  |  |  |  |
| --- | --- | --- | --- |
| 0x54 | DevID | Interval scalar | Checksum |

Check interval (ms) =

### Post All EEPROM variables

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0x55 | Length | DevID | Byte 0 | Byte 1 | … | Checksum |

### Request All EEPROM Values

|  |  |  |
| --- | --- | --- |
| 0x59 | DevID | Checksum |

## EEPROM on Arduino

|  |  |  |
| --- | --- | --- |
|  | 0x00 | 0x10 |
| 0x0 |  |  |
| 0x1 | Device ID |  |
| 0x2 | Input Devices |  |
| 0x3 | Output Devices |  |
| 0x4 | Blink scalar |  |
| 0x5 | Pulse scalar |  |
| 0x6 | Check scalar |  |
| 0x7 |  |  |
| 0x8 |  |  |
| 0x9 |  |  |
| 0xA |  |  |
| 0xB |  |  |
| 0xC |  |  |
| 0xD |  |  |
| 0xE |  |  |
| 0xF |  |  |